Arduino

Reference Language | Libraries | Comparison | Changes

## micros()

#### Description

Returns the number of microseconds since the Arduino board began running the current program. This number will overflow (go back to zero), after approximately 70 minutes. On 16 MHz Arduino boards (e.g. Duemilanove and Nano), this function has a resolution of four microseconds (i.e. the value returned is always a multiple of four). On 8 MHz Arduino boards (e.g. the LilyPad), this function has a resolution of eight microseconds.

Note: there are 1,000 microseconds in a millisecond and 1,000,000 microseconds in a second.

#### Parameters

None

#### Returns

Number of microseconds since the program started (unsigned long)

#### Example

    unsigned long time;

    void setup(){
      Serial.begin(9600);
    }
    void loop(){
      Serial.print("Time: ");
      time = micros();
      //prints time since program started
      Serial.println(time);
      // wait a second so as not to send massive amounts of data
      delay(1000);
    }

#### See also

- millis()
- delay()
- delayMicroseconds()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Share|
©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes